1.Our company located in State-level economic development zone Linyi city Shangdong province, China. The Jinlun machinery Co., ltd was initiated and established since1999 by our general manager Mr Li, We specialize in manufacturing

woodworking machinery such as log debarker, veneer peeling machine, composer, pannel saw, glue spreader, glue mixer, hot press, cold press, sander etc. It has earned more than 20 national patents and formed a whole high technique equipments and a completely set of production line. We are one of the largest professional manufactures factory in China.

葡萄牙语：

2.1.3m Veneer product line

葡萄牙语：

Log debarker

葡萄牙语：

Wood peeling machine

葡萄牙语:

**Veneer stacker**

葡萄牙语：

Debarker is used for log for round before peeling.

removing the log’s skin and straighting logs. One set debarker can supply 2 set peeling machine .it saves the original manual peeling, rounding procedure, save 5-6 human.

**Mechanical Property:**

1, increase of single and double roll’s diameter, improving the speed of remove skin .

2, single, double roll surface with chrome plating, improve wear resisting of roller.

3, the hydraulic feeding mechanism, a cutter, rapid, and feed pressure can be adjusted and display, adapt to different wood .

4, simple operation, convenient maintenance, requirements for operators and workers is not high technology

葡萄牙语：

|  |  |  |  |
| --- | --- | --- | --- |
| 英语 | 葡萄牙语 | 英语 | 葡萄牙语 |
| Type  |  | Peeling blade(L\*W\*H)  |  |
| Max.peeling length  |  | Control system  |  |
| Max.peeling diameter  |  | Motor type  |  |
| Cutting speed |  | Total power  |  |
| Peeling rate  |  | Total weight  |  |
| Wood loss rate  |  | Dimensions  |  |
| Numbers of motor  |  | FOB PRICE  |  |
| Number of cylinder  |  |  |

Peeling is the most popular plywood producing process. Back veneer thickness is about 0.6mm, core veneer and centre veneer thickness is about 1.8mm

葡萄牙语：

**Mechanical Property:**

1.The guide adds dovetail, improve the evenness of the wood

 veneer, and the veneer error is (±0.05~0.07)mm.

2.The width error of the veneer is little(±3~5mm).

3.Advanced control system, cutting thickness from 0.5 to4.2mm

4.Rotary peeling speed can be 48m/min, high efficiency.

5.Rubber roller is Nylon, long service life

葡萄牙语：

|  |  |  |  |
| --- | --- | --- | --- |
| **英语** | **葡萄牙语** | **英语** | **葡萄牙语** |
| **Type**  |  | **Peeling blade(L\*W\*H)**  |  |
| Max.peeling length  |  | Slitting blade(L\*W\*H)  |  |
| Max.peeling diameter  |  | Motor type  |  |
| Min.residual diameter  |  | Total power  |  |
| Cutting speed |  | Total weight  |  |
| Cutting thickness  |  | Dimensions  |  |
| Veneer tolerance  |  | FOBPRICE  |  |
| Numbers of motor  |  |

|  |  |
| --- | --- |
| **英语** | **葡萄牙语** |
| Type  |  |
| Power  |  |
| Veneer thickness  |  |
| Veneer size  |  |
| Staff saving  |  |
| speed  |  |
| dimension  |  |

***Welcome to visit our company for cooperation!***

葡萄牙语：

***Any time,any questions,Contact us***

葡萄牙语：