HX-350 Baby Diaper Production Line

**Function and configuration**

1. Model explanation:

350B: basic function model;

1. product specification: 4 sizes, S,M,L,XL(specify according to client)
2. 10.4“color touch-control man-machine operation interface,main parameters are clear to see.
3. design according to Europe CE standard, electric component has CE or UL certificated, equipped with safety door and emergency stop,etc safety device.
4. equipment structure is firm and reasonable,accessories is processed well,main parts which is bought outside adopt internationally known brand.
5. optional configuration: a: full servo control stacker. B: full automatic bagging sealing machine.

**Main technical parameter:**

1. product specification: 4 sizes, S,M,L,XL;
2. designed speed: 400 pieces/minute;
3. stable production speed: 250-400 pieces/minute(vary according to configuration)

(subject to M size, exclude glue machine factor)

1. Power Supply: 380V 50HZ
2. machine capacity: about 130Kw(don’t include Glue Machine power)
3. product finished product ratio: ≥97%(exclude glue machine trouble and splicing material factors)
4. product grams weight deflection: ±5%
5. weight(including pulverizer): about 35 tons.
6. machine running direction: face machine, run from Left to Right(or specify by client)
7. machine color: dark blue color;
8. machine size: (Length × width ×height): about 20 M x 2.2 M x 2.9 M (exclude crusher).