**Main parameters of ZHG-4000**

（1）Total Volume：4000L

（2）Working volume：2400L

（3）Agitating speed：5 r/min

（4）Vacuum degree：-0.08～-0.096MPa

（5）Inner size of drum：Φ1400X2600

（6）Overall size：5500X1800X2850mm

（7）Power of motor：22kW

 **Scope of supply**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name  | Specification | Material | Unit | Quantity | Note |
| Main Machine | Inner wall  | Ф1400\*2600Thickness: 12mm | SUS304 | Module | 1 |  |
| Jacket  | Ф1530\*10mm | A3 |
| Shaft | Ф245X8 | SUS304/45# |
| End Plate | Ф1530X40 | A3/SUS304  |
| Main Attachments | Frame | carbon steel25\*16 | A3 | As module | 1 |  |
| Sealing  |  | PTFE | M | 2 |  |
| Speed reducer | JZQA650-1:40 |  | PC | 1 | China |
| Motor | 22kw |  | PC | 1 | China |
| Couplings | Ф270 | 45# steel | PC | 1 |  |
| Bearing | 73263626 |  | PC |  21 |  |
| Vacuum pipe | Ф273\*5 | SUS304 | PC | 1 |  |
| Vacuum filter | Ф273\*5 | SUS304 | PC | 1 |  |
| Discharge port | Ф250 | SUS304 | PC | 1 |  |
| Temperature sensor | 0~400℃ | Stainless steel | PC | 1 |  |
| Vacuum meter | 0~-0.1Mpa | Stainless steel | PC | 1 |  |
| Electric cabinet |  | Carbon steel | PC | 1 |  |
|  | Main electric components |  | Schneider | set | 1 |  |

Delivery Date: Within 50days after receive deposit

Payment Terms: 30% by TT as deposit, 70% by TT before shipping

Warranty period: 1year after sell

FOB Shanghai Price: 34000USD.

(The price include packing and domestic transport)

Note: Two mechanical Seals as option, need extra 4000USD