**YZG-1000**

|  |  |  |  |
| --- | --- | --- | --- |
| Number | Item | Unit | Model/specification |
| 1 | Inside size of chamber | mm | 1000\*1527 |
| 2 | Outside size of chamber | mm | 1693\*1190\*1500 |
| 3 | Layers of baking shelf | pc | 6(layer space:102mm) |
| 4 | Number of drying tray | pc | 12 |
| 5 | Size of drying tray | mm | 460\*640\*45 |
| 6 | Pressure inside baking shelf pipe | Mpa | ≤0.0784 |
| 7 | Degree of vacuum | Torr | ≤30 |
| 8 | Temperature | ℃ | 30-150 |
| 9 | Weight | Kg | 800 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No | Name | Specification | Material | Quantity | Origin |
| 1 | YZG1000 Drying Chamber | YZG1000 | Inner wall as 3mm SUS304 ；Outer wall as 1.5/2mm SUS304，Jacket as 8mm Q235AFlange as 16mm Q235AInsulation layer as 50mmthick alumina silicate | 1set | Jinling |
| 2 | Drying shelf | Φ45，Φ25，Φ18 pipe | SUS304 | 1set | Jinling |
| 3 | Door |  | Outer wall SUS304, 2mm surface polished. Middle wall Q235A, 8mm, Inner wall SS304,2mm | 1set | Jinling |
| 4 | Flange |  | Carbon steel,16mm | 1set | Jinling |
| 5 | Drying tray  | 460\*640\*45mm | SUS304 thickness as 0.8mm | 12pcs | Jinling |
| 6 | Vacuum pipe |  | SUS304 | 1set | Jinling |
| 7 | Vacuum meter | 0—0.1MPa |  | 1pc | China |
| 8 | Temperature meter | 0-150℃ |  | 1pc | China |
| 9 | Handle and chain, handing wheel | Handing wheel Φ120 | SUS304 | 1set | Jinling |
| 10 | Seal |  | Silicon | 1set | China |

**FOB Shanghai Price: 6500USD**

**Delivery date: 40days after receive deposit**

**Payment terms: 30% by TT as deposit, 70% by TT before shipping**

**YZG-1400**

|  |  |  |  |
| --- | --- | --- | --- |
| Number | Item | Unit | Model/specification |
| 1 | Inside size of chamber | mm | 1400\*2054 |
| 2 | Outside size of chamber | mm | 2386\*1657\*1920 |
| 3 | Layers of baking shelf | pc | 8(layer space:102mm) |
| 4 | Number of baking tray | pc | 32 |
| 5 | Size of baking tray | mm | 460\*640\*45 |
| 6 | Pressure inside baking shelf pipe | Mpa | ≤0.0784 |
| 7 | Degree of vacuum | Torr | ≤30 |
| 8 | Temperature | ℃ | 80 |
| 9 | Weight | Kg | 1000 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No | Name | Specification | Material | Quantity | Origin |
| 1 | YZG1400 Drying Chamber | YZG1400 | Inner wall as 3mm SUS304 ；Outer wall as 1.5/2mm SUS304，Jacket as 8mm Q235AFlange as 16mm Q235AInsulation layer as 50mmthick alumina silicate | 1set | Jinling |
| 2 | Drying shelf | Φ45，Φ25，Φ18 pipe | SUS304 | 1set | Jinling |
| 3 | Door |  | Outer wall SUS304, 2mm surface polished. Middle wall Q235A, 8mm, Inner wall SS304,2mm | 1set | Jinling |
| 4 | Flange |  | Carbon steel,16mm | 1set | Jinling |
| 5 | Drying tray  | 460\*640\*45mm | SS304 thickness as 0.8mm | 32pcs | Jinling |
| 6 | Vacuum pipe |  | SUS304 | 1set | Jinling |
| 7 | Vacuum meter | 0—0.1MPa |  | 1pc | China |
| 8 | Temperature meter | 0-150℃ |  | 1pc | China |
| 9 | Handle and chain, handing wheel | Handing wheel Φ120 | SUS304 | 1set | Jinling |
| 10 | Seal |  | Silicon | 1set | China |

**FOB Shanghai Price: 9000USD**

**Delivery date: 40days after receive deposit**

**Payment terms: 30% by TT as deposit, 70% by TT before shipping**