|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1.Certificate Number | YG17XDGK0823129 | 2.Issue date | 2017-01-28 | |
| 3.Manufacturer | SINOTRUK | | | |
| 4.Serial type | HOWO | Cargo truck | | |
| 5.Chassis Category | II | 6.Type | ZZ1317N4667E1H | |
| 7.Chassis ID | 2806056 | | | |
| 8.Body color | Hot Red | | | |
| 9.VIN | LZZ1BXNF3HN125416 | 10.Fuel | Diesel | |
| 11.Engine | D10.34-50 | 12.Power(mL/kW) | 9726/249 | |
| 13.Engine ID | 160307022817 |  |  | |
| 14.Emission standard | Euro V | | | |
| 15.Steering | Steering wheel | 16.Tire | 12 | |
| 17. Tire type | 12:00R20 16PR | | | |
| 18.Distance (F/R)(mm) | 2022/2022 | 1830/1830 | | |
| 19.Wheelbase(mm) | 1800+4600+1350 | | | |
| 20.Axle load(kg) | 6500/7000/17500(dual axle) | | | |
| 21.Axle Number | 4 | 22. Plate spring(pcs) | | 11/11/12 |
| 23. Overall size (mm) | 11695/2496/3730 | 24.Total weight(kg) | | 31000 |
| 25. Tare(kg) | 11100 | 26.Towed weight(kg) | | -- |
| 27.Trailer Max.weight | -- | 31.QR code | |  |
| 28.Crew in cab(person) | 2 |
| 29.Max speed(km/h) | 102 |
| 30.Manufacture date | 2017-01-28 |
| Note:the chassis can choose semi-tall roof , height is 3125mm, or tall roof , height is 3730mm | |
| Manufacturer information:  The product have been complete tested, meet (Q/3700ZZG017-2014(HOWO )Euro IV, V truck)standard. Hereby certificate.  Chassis manufacturer: SINOTRUK  Address: Danzhuan town , JINAN, China. | | | | |