**SPARE PARTS IN CONTROL PANEL – ZLP 800**

|  |  |  |
| --- | --- | --- |
| S.No. | Name | Price IN $USD |
| 1. | Power Leakage Breaker | 7.5 |
| 2. | Fuse Protector | 2.5 |
| 3. | Intelligent Control Module | 75 |
| 4. | Launch Button (with indicator light) | 1.5 |
| 5. | Button up | 1.5 |
| 6. | Button down | 1.5 |
| 7. | Stop button | 1.5 |
| 8. | Change-over switch | 5.5 |
| 9. | Buzzer | 1.5 |
| 10. | Overtravel-limit switch | 3 |
| 11. | Aviation plug base 9 cores | 4.5 |
| 12. | Aviation plug base 5 cores | 4 |
| 13. | Aviation plug 4 cores | 1.5 |
| 14. | Rectifier block | 1.5 |
| 15. | Hand control | 2.5 |

**ACCESSORY IN HOIST – ZLP 800**

|  |  |  |
| --- | --- | --- |
| S.No. | Name | Price IN $USD |
| 1. | Pinch roller | 8.3 |
| 2. | Rope guider | 1.8 |
| 3. | Friction unit | 4 |
| 4. | Hoist box/shell | 55 |
| 5. | Steel belt | 1.5 |
| 6. | In & Out rope tube | 2 |
| 7. | Electromagnetic brake | 27.5 |
| 8. | Inner gear | 21 |
| 9. | Copper gear | 14.5 |
| 10. | Worm wheel | 8.5 |
| 11. | Oil seals | 3 |
| 12. | Motor cooling fan | 0.5 |
| 13. | Motor – ZLP 800 | 95 |
| 14. | Gear box set – complete with out motor | 200 |