**PHM-320/220**





The differences between the cold lid cup mold and the hot lid cup mold:

* The cold lid cup mold is made for two pieces. Instead the hot lid cup mold is made for three pieces; Two for the top mold.
* The hot lid cup mold has not air connections as the cold lid cup mold.
* The two pieces for the top hot lid cup mold cannot join together with any kind of subjection.

A continuación detallo las diferencias entre los moldes de tapas frías y calientes:

* Juego de moldes de tapas frías está conformado por dos piezas. Mientras que la pieza superior del molde de tapas calientes está formado por dos piezas.
* Molde base de tapa caliente no tiene conexiones de aire
* Las dos piezas del molde superior de tapas en caliente no pueden sujetarse de ninguna forma.

Adjunto fotos a continuacion / pictures attached below:





1.- tapas calientes 2.- tapas frias

