无锡振达自动化设备有限公司

Wuxi Zhenda Automation Equipment Co. , ltd

Add: No.3 district, Private Economy, Xibei, Wuxi City, Jiangsu Province T：0086-510-8313 7670 F: 0086-510-8313 5092

WEBSITE:www.zdplatform.com

Skype:misscici119 E-mail:cicizhenda@gmail.com

QUOTATION

To: Mr Fabio Ramos

E-mail: fabio_rt@hotmail.com From: cici

Currency: USD Date: 2014-8-26

cement with cast iron cover counterweight

cast iron counterweight

Model	ZLP 630
Material	Steel
Rated load	630kg
Power	220V / 50Hz / single phase
Standard Lifting Height（m）	100 meters
Surfacing	Hot galvanize
Counter weight	cement with cast iron cover
Length of suspended platform	6 meters
Ex-work Price	2806 usd / set （cement with cast iron cover）
Ex-work Price	3258 usd / set (cast iron cover )
1 SET ZLP 630 (Standard Accessories） including 1 piece electrical control box, two pieces hoist, two pieces safety lock, and counter weight 900kg, 6m platform, and suspension mechanism.

Remarks:

================================

1.Payment: USD 100% paid in advance by T/T.

Delivery time: 10 days from receipt of the payment.

Other terms: The currency rate between USD and CNY is calculated as 1: 6.15

All final price are subject to the exchange rate and may adjust accordingly