无锡振达自动化设备有限公司

Wuxi Zhenda Automation Equipment Co. , ltd

Add: No.3 district, Private Economy, Xibei, Wuxi City, Jiangsu Province T：0086-510-8313 7670 F: 0086-510-8313 5092

WEBSITE:www.zdplatform.com

Skype:misscici119 E-mail:cicizhenda@gmail.com

QUOTATION

To: Mr Jose Rosas

E-mail: ppros2@yahoo.com From: cici

Currency: USD Date: 2014-11-21

counterweight: cement with cast iron cover

Model	ZLP 630
Material	Aluminum Alloy
Rated load	630kg
Power

220 v/ single phase / 60 Hz

220V/ single phase /60Hz

Standard Lifting Height（m）	100m
Surfacing

Plastic coating

Counter weight

Cement with cast iron cover 900kg

Length of suspended platform	6 m
Ex-work price	USD 2696 ( 1 set )
FOB Shanghai Port Price	USD 2990 ( 1 set )
1 SET ZLP630 (Standard Accessories） including 1 piece electrical control box, two pieces hoist, two pieces safety lock, 100 meters electric cable , 400 m steel wire rope and counter weight 900kg, 6m platform, and suspension mechanism.

Model	ZLP 800
Material	Aluminum Alloy
Rated load	800kg
Power

220 v/ single phase / 60 Hz

220V/ single phase /60Hz

Standard Lifting Height（m）	100m
Surfacing

Plastic coating

Counter weight

Cement with cast iron cover 1000kg

Length of suspended platform	7.5 m
Ex-work price	USD 2859 ( 1 set )
FOB Shanghai Port Price	USD 3153 ( 1 set )
1 SET ZLP800 (Standard Accessories） including 1 piece electrical control box, two pieces hoist, two pieces safety lock, 100 meters electric cable , 400 m steel wire rope and counter weight 1000kg, 7.5m platform, and suspension mechanism.

Remarks:

================================

1.Payment: USD 100% paid in advance by T/T.

Delivery time: 10 days from receipt of the payment.

Other terms: The currency rate between USD and CNY is calculated as 1: 6.1

All final price are subject to the exchange rate and may adjust accordingly