|  |  |
| --- | --- |
| Name | Veneer composer |
| Veneer length | Less than 2500mm(3/4pcs veneer compose) |
| Veneer width | Less than 1300mm |
| Veneer thickness | 0.8-4.0mm |
| Total power | 32kw |
| Overall size | 10000mmx2400mmx2400mm |
| Capacity | 3000-4000pics |
| Video Link | <https://www.youtube.com/watch?v=HqkJbX_QSCg&feature=youtu.be> |
| Staff saving | Save 10 staff |

Wood veneer composer machine is used to compose core veneer for plywood. The benefit is staff saving. The output of this machine is about 11 staff work per day(8 hours). Edge of the wood veneer is cut by automatic cutter which is more straight by man-made. Same direction wood fiber makes plywood stronger.

