|  |  |  |  |
| --- | --- | --- | --- |
| Código  | Denominación  | U/M | Cantidad |
|  | Drinking Systems for floor breeding, integrated by : |  |  |
| 4039 | Wu 3 mtr, aluminum 15x4022,15x4612-01 | U | 3600 |
| 3206-00 | Pressure regulator mid 22 mm( 450 mm br. u) -yellow | U | 120 |
| 4255-00 | Flush-breather unit-yellow | U | 240 |
| 4376-00 | Hanger bracket- yellow | U | 14400 |
| 4444 | Connection set for shocker-wire | U | 120 |
| 4429 | Shockerwire 1.5 mm galv. | M | 12000 |
| 4417 | Handwinch 600 kg with support | U | 120 |
| 4432 | Guide pulley | U | 120 |
| 4431 | Ceiling pulley | U | 3800 |
| 4426 | Cable ø 4mm on coil 100m | M | 12000 |
| 4434 | Plastic rope | U | 16000 |
| 4436-00 | Clamping screw- yellow | U | 4000 |
| 4433 | Cable clamp 3/16" | U | 4000 |
| 9231 | Waterfilter ¾",100 Mikron |  | 40 |

Características técnicas Sistema dosificador de Medicamentos Liubing (Water Supply)

|  |  |  |  |
| --- | --- | --- | --- |
| 4265 | Main water Supply with water Filter, watermeter , pressure , reduce valve and and medicator art 4238-1 with by pass. | U | 120 |
| 4248 | Mixer 60 lts .230 volt, 60 hz | U | 120 |