

Log debarker machine

|  |  |
| --- | --- |
| Model | YPM60 |
| Motor (KW) | 7.5\*2 |
| Debarking diameter (cm) | 5-60 |
| Capacity(ton/h ) | 2-3T bark/hour |
| Peeling rate | >95% |
| Timber lose rate | <2% |
|  |  |



Wood chip machine

Quantity: 8-15Tons/hour

Max log diameter: no less than 300mm

Chip size: 2-5cm







|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Model | Power (kw) | Capacity (t/h) | Product spec (mm) | Weight (t) | Dimension (mm) |
| XGJ560 | 90+3+0.25+1.5 | 1-1.5 | Φ4-12 | 5.3 | 2600x1300x2300 |
| XGJ720 | 160+3+0.25+2.2 | 1.5-2 | Φ4-12 | 9.5 | 2900x1300x2400 |
| XGJ850 | 220+4+0.55+3 | 2-3 | Φ4-12 | 14. 2 | 3300x1400x3100 |
| XGJ920 | 315+5.5+3+0.55+3 | 3-4 | Φ4-12 | 18 | 3800x1680x3400 |
| XGJ1050 | 360 | 5-6 | Φ4-12 | 2 4.5 | 3800x1880x3500 |

Wood Pellet Machine has filled the country blank in vertical feeding for ring die pellet mill and reached the international advanced level.  
Wood Pellet Machine is mainly applicable for difficult molding materials with low adhesion rate, for example rice husk, sunflower husk, peanut shell and fruit shell; branch, stem, bark and other wood waste; a variety of crop stalks; rubber, cement, ash and other chemical materials.  
  
Wood Pellet making Machinery can be used in feed mill, wood processing plants, fuel plants, fertilizer plants, chemical plants etc. Since it requires less investment and yield quicker result and that no risk. Vertical Ring-die Wood Pellet Machine for sale is an ideal dense compression molding equipment.