JIN LUN machinery Co., ltd

Our company located in State-level economic development zone Linyi city Shangdong province，The Jinlun machinery Co., ltd was initiated and established since 1999 by our general manager Mr Li, We specialize in manufacturing woodworking peeling machinery . It has earned more than 20 national patents and formed a whole series of high-technique equipments and a completely set of production line ,such as 4 feet ,8 feet ,10 feet of peeling machine for spindle and spindleless. We are one of the largest professional manufactures factory in China . Our machines own the highest domestic market share and exported to more than 20 countries, such as Vietnam, Thailand, Indonesia, Malaysia, Philippines, India, Pakistan, Turkey, Russia, South Korea, Brazil, Paraguay, Nigeria and so on .

Welcome to visit our company for cooperation.

Wood Peeling machine:

Peeling machine is the main equipment for the production of plywood. Peeling machine divided into spindle peeling machine and spindleless peeling machine.digital servo control technology is also applied to the peeling machine .CNC peeling machine not only improve the quality and accuracy of veneer but also greatly improve the veneer output .

Mechanical Property :

1. The guide adds dovetail, improve the evenness of the wood veneer, and the veneer error is (±0.05~0.07)mm.

2. The width error of the veneer is little(±3~5mm).

3. All motor are national standard.

4. Automatic setting seam, alleviate the pressure of the spiral cutting, to increase the service life of the bearing.

5. Advanced control system, cutting thickness from 0.5 to4.2mm

6. Bearing seat with position pin, easy maintenance.

7. Rotary peeling speed can be 48m/min, high efficiency.

8. Rubber roller is Nylon, long service life.

9. Quality standards Q/FJJ002-2007

Log debarker

log debarker is used for log for round before peeling. And it is suitable for the eucalyptus, pine, cotton wood .with principle of peeling, removing the log’s skin and straighting logs. hydraulic driven feed mechanism,can quickly, efficiently put log removal of bark, round. One set debarker can supply 2 set peeling machine .it saves the original manual peeling, rounding procedure, save 5-6 human.

log debarker features：

1, increase of single and double roll’s diameter, improving the speed of remove skin .

2, single, double roll surface with chrome plating, improve wear resisting of roller.

3, the hydraulic feeding mechanism, a cutter, rapid, and feed pressure can be adjusted and display, adapt to different wood

4, simple operation, convenient maintenance, requirements for operators and workers is not high technology