无锡振达自动化设备有限公司

Wuxi Zhenda Automation Equipment Co. , ltd

Add: No.3 district, Private Economy, Xibei, Wuxi City, Jiangsu Province T：0086-510-8313 7670 F: 0086-510-8313 5092

WEBSITE:www.zdplatform.com

Skype:misscici119 E-mail:cicizhenda@gmail.com

QUOTATION

To: Oswaldo Julian Jaimes Diaz

E-mail: o_jaimes0811@hotmail.com From: cici

Currency: USD Date: 2015-05-27

counterweight: cement with cast iron cover

Model	ZLP 630
Material	Steel
Rated load	630kg
Power

230 v/ Three phase / 60 Hz

220V/ single phase /60Hz

Standard Lifting Height（m）	100m
Surfacing

Plastic coating (yellow)
Counter weight

Cement with cast iron cover 900kg

Length of suspended platform	6 m
Ex-work price	USD 2025 ( 1 set )
FOB Shanghai Port, China Price	USD 2265 ( 1 SET)
CIF Callao	USD 2550 (1 set)
1 SET ZLP 630 (Standard Accessories） including 1 piece electrical control box, two pieces hoist, two pieces safety lock, 100 meters electric cable , 400 m steel wire rope and counter weight 900kg, 6m platform, and suspension mechanism.

EXW: USD 805 (2 PCS)

Remarks:

================================

1.Payment: USD 100% paid in advance by T/T.

Delivery time: 10 days from receipt of the payment.

Other terms: The currency rate between USD and CNY is calculated as 1: 6.2

All final price are subject to the exchange rate and may adjust accordingly