无锡振达自动化设备有限公司

Wuxi Zhenda Automation Equipment Co. , ltd

Add: No.3 district, Private Economy, Xibei, Wuxi City, Jiangsu Province T：0086-510-8313 7670 F: 0086-510-8313 5092

WEBSITE:www.zdplatform.com

Skype:misscici119 E-mail:cicizhenda@gmail.com

QUOTATION

To: Armando Dias

E-mail: travangulo@sapo.pt From: cici

Currency: USD Date: 2015-06-03

counterweight: cement with cast iron cover

Model	ZLP 800	ZLP 800
Material	Aluminum Alloy	Steel
Rated load	800 kg	800 kg
Power

230 v/ single phase / 50 Hz

220V/ single phase /60Hz

230 v/ single phase / 50 Hz

Standard Lifting Height（m）	100m	100m
Surfacing

Plastic coating	Hot galvanized
Counter weight

Cement with cast iron cover 1000kg

Cement with cast iron cover 1000kg

Length of suspended platform	7.5 m	7.5 m
Ex-work price	USD 2677 ( 1 set )	USD 2919 (1 SET)
FOB Shanghai Port ,China	USD 2919 ( 1 SET)	USD 3159 (1 SET)
1 SET ZLP 800 (Standard Accessories） including 1 piece electrical control box, two pieces hoist, two pieces safety lock, 100 meters electric cable , 400 m steel wire rope and counter weight 1000kg, 7.5m platform, and suspension mechanism.