无锡振达自动化设备有限公司

Wuxi Zhenda Automation Equipment Co. , ltd

Add: No.3 district, Private Economy, Xibei, Wuxi City, Jiangsu Province T：0086-510-8313 7670 F: 0086-510-8313 5092

WEBSITE:www.zdplatform.com

Skype:misscici119 E-mail:cicizhenda@gmail.com

QUOTATION

To: Mario Navarrete

E-mail: comitenatura@gmail.com From: cici

Currency: USD Date: 2015-6-12

counterweight: cement with cast iron cover

Model	ZLP 500
Material	Aluminum alloy
Rated load	630kg
Power	110 v/ single phase / 60 Hz

Standard Lifting Height（m）	100m
Surfacing

Plastic coating

Counter weight

cement with cast iron cover

Length of suspended platform	5 m
Ex-work price	USD 2675 ( 1 set )
FOB Shanghai Port,China	USD 2915 (1 SET)
1 SET ZLP 500 (Standard Accessories） including 1 piece electrical control box, two pieces hoist, two pieces safety lock, 100 meters electric cable , 400 m steel wire rope and counter weight 750 kg, 5m platform, and suspension mechanism.

Remarks:

================================

1.Payment: USD 100% paid in advance by T/T.

Delivery time: 10 days from receipt of the payment.

Other terms: The currency rate between USD and CNY is calculated as 1: 6.2

All final price are subject to the exchange rate and may adjust accordingly