|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model** | **Ice weight & ice dimension** | **Ice making time** | **Ice cans & water tank** | **Capacity / shift** | **Capacity / 24hrs** | **Germany Bitzer Compresor** | **Cooling system** | **FOB price** |
| MB10 | 5 kg / 80\*165\*500 mm | 4.8 hours | Stainless steel 304 material | 40 pcs block ice | 200 pcs = 1 tons | 4 HP | Air cooling system | **$ 7,220 USD** |
| MB50 | 10 kg / 100\*205\*610 mm | 6 hours | 125 pcs block ice | 500 pcs = 5 tons | 28 HP | Water cooling system | **$ 19,150 USD** |
| MB60 | 150 pcs block ice | 600 pcs = 6 tons | **$ 23,690 USD** |
| MB100 | 25 kg / 120\*360\*750 mm | 8 hours | 134 pcs block ice | 402 pcs = 10 tons | 2 \* 28 HP | **$ 39,240 USD** |