Introduction

Production Workshop

Machine Model

Technical Details

Machine lesson

Payment & Delivery

Please Scan Me!

Zhejiang New Debao Machinery was established in 1999 and has become the biggest paper cup forming machine manufacturer in China through its own production technology for the high performance paper cup forming machine.The best quality control and the customer service enables the company to become a leader in this line. New Debao currently exports paper cup forming machine to 40 countries around world including (South)east Asia, Europe, Oceania, and North America and the quality of its products and services are highly recognized by the worldwide customers.

The customer has been certified by carious domestic and international certification bodies such as ISO9001,CE. Based on 17 years of experience in producing paper cup forming machine, New Debao consistently strives to innovate and develop relevant and new technologies in order to become the worldwide best paper cup production machinery manufacturer.

Machine installation workshop

30 sets/month

Machine adjust & test workshop

Normal speed paper cup machine workshop

Output: 120 sets/month

60 sets CNC lathe parts forming workshop

Coffee Bar

|  |  |  |  |
| --- | --- | --- | --- |
| Model | DEBAO-C22 |  |  |
| Weight | 1600 kg |  |  |
| Packing specifications | 3000\*1600\*1900mm |  |  |
| Total Power | Three-Phase 380V, 3.8/8KW |  |  |
| Air supply requirement | 0.4-0.6Mpa, 0.5Cube/min |  |  |
| Capacity | 45-55 Cups/min |  |  |
| Paper specification | Single PE |  |  |
| Paper grams | 150-250g/m2 |  |  |
| Paper cup specifications | (D1)Φ60-128mm (H)45-180mm(D2)Φ50-97mm (h)4.5-10mm |  |  |

DEBAO-C22 paper cup machine is multi-station machine. It has continuous automatic procedure like feeding, sealing, oil-filling, bottom forming, heating, knurling,curling,unloading,etc.It is widely used for High height cups, popcorn cups,snack cups. The machine production capacity can up to 30-40cups/min for 22oz cups. If your cup is Double PE Coated paper cups. We recommend you DEBAO-2C22 paper cup machine with ultrasonic sealing.

DEBAO-C22 front frame is a inclined, so paper cups can drop into plastic hole more easily.

This design also save more electricity when machine working and also solve the problem of paper jam.

Korea imported Optical Axis, Flexible& Stable, Best quality

Machine cup side sealing mould is a flat. It can help cups sealing more well of its side. And less rate of water leaking.

3 moulds turn-plate on the machine are Aluminum material.

Compared with iron made turn-plate, Aluminum turn-plate is less weight. There’s less pressure when machine driving the turn-plate up and down.

Besides, machine can work faster, and machine working life will be longer.

We use 4 gears for machine main driving system. gears will be higher precision. And 3 rows of chains for assistant drive.

Machine work more stable.

Machine electric box is designed on the machine, it can make your workshop more clear. The electric wire won’t be a mass on the ground.

It will be more safety for your worker and save more work place for more machine

The material of this board,we use Nodular cast iron has much more impact and fatigue resistance due to its nodular graphite inclusions.

Compared with iron material board, The plate won’t get out of shape in long time running

Q1:On this machine, can I make all size as I like?

R1:Because the machine have a range of cup size. So it can not make any size as you like?

For machine DEBAO-C22, It can make from 16oz---32oz.

Q2: One machine how many size I can make?

R1: For new skilled customers,we recommend one machine one size. You don’t need change moulds. Changing mould and adjust may takes 2-3 days or more for new users. However, when you get experienced, we can reconsider to add extra moulds.

Q3: How can I start?

R1: We need to know:

1. what size of paper cup you want make? The paper is single PE or double PE? What thickness is the paper?

(Or you can send me the sample,we can make cup drawing for you including all information.)

1. How’s output for day for each size?
2. Your cup is single PE or double PE?

After comfirmed the size, and received deposit, We will start production soon.

Q4:If I change Paper in the future? If the mould need to Change?

R4: Sometimes customer may change the paper thicknees for same size. If the paper thickness is similar thickness. you can change it. If thickness is >40gsm difference, you may need change some spart parts.

Q5: When my machine arrived, what work should I do to start machine? How’s overseas engineer service?

R1: When new machine arrived, please link electric according the video or manual book guidance. If your machine is ultrasonic welding. Pls link air compressor also. If you need engineer overseas service, we can arrange engineer to your factory help you start machine and train your works. You need to arrange for 2-ways flight tickets, hotel, eating,translation and 100 USD per day for salary.

**Warranty:**We warranty 1 year for machine mechanical part & electrical part, (excluding easy wearing spare parts). The damage by customer misuse, improper handling, neglectful maintain, force injury and other reasons are beyond our responsibility. So please operate machine according to the manual book or videos.

**Payment:** 100%T/T. 30%T/T paid as the deposit, 70%T/T paid before shipment.

**Delivery time**: 90 days

**Package:** Standard wooden case, 1 Set machine in one case

**Loading port:** Ningbo

Contact:Jane Chan Email: Sale4@debaochina.com

Whatsapp/Mobile: 008613958815566