|  |  |  |  |
| --- | --- | --- | --- |
| SPRAY BOOTHS IMPORTER | | 2017 | |
|  |  |  |  |

SPECIAL SPRAY BOOTH REQUIREMENT

COMPANY**： METCHAL I** DATE：**02.02.2017**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NO. | ITEM | DESCRIPSION Spray booth | | | | | | | | | | | | | | |
| 1 | INSIDE SIZE | Total **7000x4000x3000**(LxWxH)mm / | | | | | | | | | | | | | | |
| If you are not sure the size of spray booth, please fill in the size of the goods which will be painted. | | | | | | | | | | | | | | | | |
| 2 | SIZE OF GOODS | 2 section: (L) mm | | | | | | | | | | | | | | |
| 3 | WALL PANEL INSULATION | ROCK WOOL □X | | | | | EPS □ | | | | | | | PU □ | | |
| 4 | ROOF PANEL | ROCK WOOL □X | | | | | | | | | | EPS □ | | | | PU □ |
| 5 | MAIN DOOR INSULATION | ROCK WOOL □X | | | | | EPS □ | | | | | | | PU □ | | |
| 6 | INTAKE AND EXHAUST AIR CABINET POSITION | RIGHT □X | | | LEFT □ | | | | | REAR □ | | | | | | TOP □ |
| 7 | MATEIRAL OF CABINET FRAME | ALUMINIUM ALLOY □ | | | | | | QUADRATE STEEL □X | | | | | | | | |
| 8 | WITH BASEMENT | UP GROUND □ | | | | | | DOWN GROUND □X | | | | | | | | |
| 9 | WITHOUT BASEMENT | PIT □X | EXHAUST FROM SIDE WALL□ | | | | | | | | | | EXHAUST FROM REAR WALL□ | | | |
| 10 | GRILLE | ALL □X | | 3 ROWS □ | | | | | 2 ROWS□ | | | | | NO GRIDS □X | | |
| 11 | RAMP | RAMP OUT□ | | | | | RAMP IN □ | | | | | | | NO RAMP □X | | |
| 12 | BURNER | DIRECT(GAS) □ | | | | | GAS □X | | | | | | | OIL □ | | |
| SINGLE STAGE □ | | | | | | | | | 2 STAGE □X | | | | | |
| 14 | ACCESS DOOR STYLE | ONE DOOR □X | | | | DRIVE THROUGH □ | | | | | | | | | ELECTRICALSHUTTER  □ | |
| 15 | DOOR COLOR | WHITE □ | | | | | ORANGE □ | | | | | | | BLUE □X | | |
| 16 | CABIN COLOR | WHITE □ | | | | | ORANGE □ | | | | | | | BLUE □X | | |
| 17 | SIDE LIGHTS | VERTICAL □X | | | | HORIZONTAL □ | | | | | | | | | NO □ | |
| 18 | CONTROL PANEL | WITH □X (All components with CE) | | | | | | | | | WITHOUT □ | | | | | |
| 19 | VOLTAGE AND FREQUENCY OF POWER | 3 PHASE x , 220/380 V, 5 0 Hz(eg: 3phase x 380V,50HZ) | | | | | | | | | | | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| SPRAY BOOTHS IMPORTER | | 2017 | |
|  |  |  |  |

|  |  |  |
| --- | --- | --- |
| 20 | SPECIAL REQUIREMENT | 1. illumination min .1200 lux/m2, 2. service door 2000x800 3. inverters for each electric motors, , 4. air intake/exhaust pipes 16 pcs 5. Gas burner 6. air flow 30000 m3/h 7. Optional give price version with EPS |