QUOTATION

To: Master Box Embalagens Especiais Ltda

Attn: Jose

Date: May 18th, 2017

HM-650A Automatic Gluing Machine

|  |  |  |  |
| --- | --- | --- | --- |
| Picture | Specification | Unit/Price FOB SHENZHEN,CHINA | Delivery Date |
| Gluing machine | Paper Width Size:80-600mm | USD7120/ set | 15days |
| Paper Thickness:80-200gsm |
| Speed:7-40pcs/min |
| Voltage:380V |
| Power:6.6KW |
| Net Weight: 1100kg |
| Measurement:6350\*1650\*1100mm |
| **Function and features:**Automatic gluing machine is suitable for feeding and gluing the paper which is for making book cover, rigid box, set up box, etc.It has the function of automatic feeding paper and gluing, automatic temperature control and 24-hours timer. The draft fan under the assembly lines prevents cover paper from curling and bubbling. Feeder absorption and feed are applied, which contribute to the characteristic of steady and quick paper conveyance.Hot melt adhesives (animal adhesives) are used for health and environmental protection, and they also save cost because of the recycle system and the adjustable speeds. Ps:1, Standard working table is around 5 meters 2. 7m, 9m ,11m working table can be customized per to the customer's need. 3, Remodel for white glue( Optional)4. Run & Stop Function( Optional) |

HM-40 Corner Pasting Machine

|  |  |  |  |
| --- | --- | --- | --- |
| Picture | Specification | Unit/Price FOB SHENZHEN,CHINA | Delivery Date |
| HM-40 | Box Min,Size:40x40x10mm | USD1330/ set | 10days |
| Max.Size: Not limit |
| Speed: 20-40pcs/min |
| Voltage:220V |
| Power:0.4kw |
| Tape Width:19mm |
| Tape Length(Max.): 30mm |
| Net Weight:170kg |
| Measurement:800x500x1400mm |
| **Function and Features:**HM-40 is a machine with function of pasting the four angles of the inside box(grey board box) of Rigid box manually. Saving supplies with using hot melt tape.Boxes pasted by it can be with features of stable, smooth & elegant. It is the indispensable equipments for box making.**Raw material related: PVC TAPE**QQ图片20140902100110 20140916_091156**QQ图片20140915182433 20140916_091102** |

HM-500A Automatic Box Forming Machine

|  |  |  |  |
| --- | --- | --- | --- |
| Picture | Specification | Unit/Price FOB SHENZHEN,CHINA | Delivery Date |
| 4G$W4XO7H4`M}IOOD@JE}ZW | Box Max size:500x400x120mm | USD13970/ set  | 15days |
| Box.Min size:80x60x10mm |
| Paper Folding-in Size: 10-60mm |
| Working Speed: 15-20pcs/min |
| Voltage:AC220V |
| Power:2.2kw |
| Net Weight: 900kg |
| Machine Dimension:900x800x2960mm |
| **Features and functions:**This machine is available in wrapping and folding the paper edge for rigid box, fancy box, and cardboard box, etc. 1. It applies servo motor and PLC control.
2. The adjusting of the 4 sides is controlled by screw, thus more precise and easier.
3. The electric parts apply international brand. Low malfunction and high accuracy.
4. With alarm functions display on screen.
5. With emergency stop switch.
6. When the machine is working, the maximum height could be 2200mm.

Design 1Design 2 |

HM-YP300B Box Pressing Machine

|  |  |  |  |
| --- | --- | --- | --- |
| Picture | Specification | Unit/Price FOB SHENZHEN,CHINA | Delivery Date |
| C:\Users\sal11\AppData\Roaming\Tencent\Users\1019307470\QQ\WinTemp\RichOle\Z7Z@IAJ$}B{U)2LZZ73O_5U.png | Box Max size:250x200x80mm | USD1250/set | 10days |
| Box.Min size:50x50x10mm |
| Ideal Box size.(Max):250x150x60mm |
| External Pressure:0.5-0.8Mpa |
| Downward Pressure:160-220kgf |
| Side Pressure: 120-140kgf |
| Upward Pressure: 40-60kgf |
| Voltage: AC220V |
| Power: 20w |
| Net Weight: 85kg |
| Machine Dimension: 800x600x1450mm |

**Note:**

1. Above price is valid for 30days, and it doesn’t include the installation charges
2. If customer want manufacturer to send technician to install and train the operation. The customer should bear the come and back ticket fee, housing, eating and transporation fee in customer local side.
3. Price is only for standard. Other special requirements should discuss further.
4. Guarantee: One year
5. Package: Vacumm packing + Wooden Case