**Landscaping Grass**

TYPE 1: Legend Grass (Oasis)

YARN: Tencate Oval8800



DTEX: PE8800+PP4400

COLOR: Straight (field green and lime green)

+ thatch (yellow and green)

Or (coffee and lime green)

PILE HEIGHT: 30-45mm

GUAGE: 3/8”

STITCH RATE: 14-18stitches/10cm

DENSITY: 14700-18900stitches/square meter

WARRANTY: 10 years

TYPE 8: MagicGrass3



YARN: Four-tones color grass

DTEX: PE&PP12000

COLOR: Straight (field green and lime green)

+thatch (coffee and lime green)

PILE HEIGHT: 20-40mm

GUAGE: 3/8”

STITCH RATE: 14-18stitches/10cm

DENSITY: 14700-18900 stitches/square meter

WARRANTY: 7 years

TYPE 9: MagicGrass4



YARN: Four-tones color grass

DTEX: PE&PP10500

COLOR: Straight (field green and lime green)

+thatch (yellow and green)

PILE HEIGHT: 20-40mm

GUAGE: 3/8”

STITCH RATE: 14-18stitches/10cm

DENSITY: 14700-18900 stitches/square meter

WARRANTY: 7 years