Shandong Huatong Hydraulic Pressure Machinery Co.,Ltd

山 东 高 唐 华 通 液 压 机 械 有 限 公 司

20130910

Quotation of QT7-25Semi-automatic Block Making Machine
NO.	Name	QTY	Price(USD)	Note
1	QT7-25Block Making Machine	Main Machine	1set	26300

Concrete Feeder	1set
Mould	1set
Pallets Feeder	1set
Pallets Conveyor	1set
Belt conveyor (6m)	1set
2	Mixing Machine	JS500 mixing machine	1set	6000	Two shafts
3	Free Parts	Pallets	15Pics	/
Carts	4sets	/
Ex-Store price	32300
(One 40 HQ Container ) FOB (Qingdao port)	33500
CNF Dammam port	35800
Optional Parts	Colour Feeder	1set	2600	For Paver
Pallet(1100x710x30mm)	1500Pics	15000
Notes:
I.Installation and Training:We will send technicians to buy's factory to guide installation training.Buyer is responsible for air-ticket,visa,food,accommodation,transportation and security. It is free in 10working days (50USD /person/day for extra days).
II.Payment Terms: 30% as advance paid by T/T,70% before delivery by T/T or by LC at sight.
III. Quotation Validity:60days.
IV.Delivery Time:25-30days
V.Guarantee Time:1 Year

General Introduction of QT7-25Semi-automatic Block Making Machine:

QT7-25Semi-automatic Block Making Machine(semi-automatic means that the machine is operated by one worker through some handles.But all processes are finished by the machine itself.)

QT7-25(7 stands for the production of hollow blocks like 390x190x190mm is 7 pieces every mould,and 25stands for every cycle needs 23-25seconds).

QT7-25Semi-Automatic Block Making Machine:JS500mixer(two shafts and compulsion) + Conveyor belt(6 meters)+Concrete Feeder+Main Machine+Palltes Feeder+4 Trolleys+15 Pics of pallets

Main Technical Specifications
Standard	JC/T920-2003
Vibration Frenquency	3800 cycles/minute
Vibration Pressure	70KN
Production/mould	Hollow block (390x190x190mm) 7 pics/mould
Hollow block（245×115×90mm) 20 pics/mould
Solid brick (240×115×53 mm) 36 pics/mould
Paver brick（200×100×60mm）18 pics/mould
Cycle Time	16-25seconds
Production/day(8hours)	Hollow Block(390×190×190 mm) 8100-8800 pieces
Hollow Block (245×115×90mm) 23000-25000pieces
Solid Brick (240×115×53mm) 45000-60000pieces
Paver Brick (200×100×60mm) 21000-23000pieces
Power	25.8KW
Water Consumption	4-8T
Number of workers	8-10worker
Space of Ground	4200㎡
Gross Weight	7T
Machine Dimension	3150×1900×2930mm
Main materials	Cement,crushed stone dust,gravel,sand,coal fly ash,iron/aluminium dust,crushed cinder and some industrial wastes
Products of machine	Hollow blocks,Solid bricks,Pavers,Kurbstones,Slope blocks,slabs, interlock bricks and so on.
Main Features:

QT7-25semi-automatic is the classic one of our machine,which has about 10 years history.It is simple,strong and easy to operate.This kind of machine has the following advantages:

Multifuctions:The machine can be used to make different products with different moulds,like hollow blocks,solid bricks,pavers,Kurbstones and so on.

Power-saving:when the machine is working,only the host machine is always be on,other parts only works at regular intervals.

Quick speed:The under-part and upper-part of mould inserts and pulls out quickly with high-powered hydraulic pump.Meanwhile,all the processes like moulding materials into blocks and preparing materials are finished at the same time.And the pallets moving is quick.

Easy operation:The host machine is operated by one person,and other processes will be completed automatically by electronics.Because the pressure of viberating is high,the materials needs less water.So the machine still can work under low temperature.

High quality of mould:Mould is an important part of machine.The steel is standard materials for making moulds.We have many procedures like adding carbon and boron,back fire for three times, polishing,and so on.And the geomitry of the moulds is standard too.